Plan for the viewing and cleaning walk-through is to do the following:
1) Execute SeriesSEE and go through turning series on/off and window sizing and overlap (5-10 min)
2) Use "Conditional" button to remove spikes from PM-3 and 20-2-1 spikes (5 min)
3) Use "Hyperdata" to continue removing smaller spikes in 20-7 wlevs (5 min)
4) Gapfill missing data in 20-7 wlevs with linear interpolation (5 min)
5) Use "SimpleQ" to simplify 20-8 pumping (5 min)
6) Offset 20-7 and PM-3 wlevs
7) Use "Compare" button to 
  a) add PM-3 and 20-7 wlevs with differing collection intervals, 
  b) convert 20-7 BP from MB to PSI, 68.95 Mb = 1 psi
  c) subtract converted 20-7 BP from 20-7 wlevs (10 min)
8) Use "Subtotal" button to convert PM-3 wlevs to daily averages (5 min)
